|  |  |
| --- | --- |
| Juan de la Cierva 2  08339 Vilassar de Dalt  Barcelona-Spain  P.O. Box 75  +34 937 539 630  Cif. ES A 08089633  www.brendle.es |  |

***TECHNICAL INFORMATION***

***«FAMILIA\_PRODUCTO»***

***PRODUCT: «nombre\_producto»***

***DESCRIPTION:***

*«nombre\_producto» is a «familia\_producto\_minusculas» ink for application by «metodo\_aplicacion» on «sustrato\_aplicacion». After firing it produces a metallic layer with a «bright\_matt» «tono\_color\_cocido» tone«frase\_mw»*

***TECHNICAL SPECIFICATIONS:***

*Viscosity: «viscosidad» Pas. 85°C*

*Consistency: «Consistencia» viscosity*

*Shelf Life: «Shelf\_life» at 20°C*

*Colour: «Color\_crudo»*

*Substrate: «Sustrato\_aplicacion»*

*Application: «Metodo\_aplicacion»*

*Screen Type: Metallic screen, 320-400 Mesh*

*Screen Temp.: 70-85 ºC*

*Dilution: This product is not meant to be diluted*

*Firing Temp.: «temperatura\_coccion»°C according with the total firing time*

***STORAGE:*** *Store in a cool, dry place*

***WAY OF USE:*** *Use safety gloves. Place on the heated screen until the product melts. Apply on the desired surface by «metodo\_aplicacion».*